(footprint "S-PVSON-N8"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -10.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "b7a8d5fd-fbf1-49fc-8003-bdc455cce47f")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "S-PVSON-N8"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "dd9133fa-a675-402b-a301-1b7e30eb36ed")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c237be81-ee25-4d9d-b945-db6b3c23d990")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e259358f-1feb-40c5-8da1-333694c0d01b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.575 1.575)
		(end -1.575 1.225)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "02cc6b00-6ca8-4b5e-b2ad-7f10defcb952")
	)
	(fp_line
		(start -1.575 1.575)
		(end -1.225 1.575)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "615ab2be-ea76-4bde-9a96-1eefa6ba63ae")
	)
	(fp_line
		(start 1.575 -1.575)
		(end 1.225 -1.575)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3a62d91a-4419-46d5-9d57-be4a0d945246")
	)
	(fp_line
		(start 1.575 -1.225)
		(end 1.575 -1.575)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "08ff7c18-14ad-4f64-b7c9-7de4e313fc6f")
	)
	(fp_line
		(start 1.575 1.575)
		(end 1.225 1.575)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "4359c3e4-473c-4ab4-b899-b5b8dea9ec1e")
	)
	(fp_line
		(start 1.575 1.575)
		(end 1.575 1.225)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "39f0ceec-9912-4683-9242-0e0cea6246c4")
	)
	(fp_poly
		(pts
			(xy -1.597685 -1.7) (xy -1.397685 -2) (xy -1.797685 -2)
		)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "0923c9e8-5b6e-4e6f-8fa6-36217693eb5f")
	)
	(fp_rect
		(start -0.125 -0.125)
		(end -0.775 -1.125)
		(stroke
			(width 0)
			(type solid)
		)
		(fill yes)
		(layer "F.Paste")
		(uuid "bfd9f2dd-5b2f-40f7-97aa-8ff4781daa88")
	)
	(fp_rect
		(start -0.125 0.125)
		(end -0.775 1.125)
		(stroke
			(width 0)
			(type solid)
		)
		(fill yes)
		(layer "F.Paste")
		(uuid "0306551e-dbb4-4fc9-9448-c4449d1adc18")
	)
	(fp_rect
		(start 0.125 -0.125)
		(end 0.775 -1.125)
		(stroke
			(width 0)
			(type solid)
		)
		(fill yes)
		(layer "F.Paste")
		(uuid "b35a2ca8-c436-44cf-a9d3-764c6c8b4386")
	)
	(fp_rect
		(start 0.125 0.125)
		(end 0.775 1.125)
		(stroke
			(width 0)
			(type solid)
		)
		(fill yes)
		(layer "F.Paste")
		(uuid "3f3cfacf-29df-4500-8f2b-a6d3d9195b1c")
	)
	(fp_rect
		(start -1.575 -1.575)
		(end 1.575 1.575)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "8cd17b04-9f6a-469d-a878-b3a127e5947c")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "bb2f483d-8636-4b1e-88a0-b098dc8be1ea")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -1.475 -0.975)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_left bottom_left)
		(uuid "0d744433-77a1-4c3b-88ef-9e630f1c4388")
	)
	(pad "2" smd roundrect
		(at -1.475 -0.327)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_left bottom_left)
		(uuid "1206d3d0-5a28-4e8d-a48d-d4fc41488a4c")
	)
	(pad "3" smd roundrect
		(at -1.475 0.327)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_left bottom_left)
		(uuid "99179aa0-7d4f-472e-bc7c-5a9969d31f22")
	)
	(pad "4" smd roundrect
		(at -1.475 0.975)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_left bottom_left)
		(uuid "3b9f98ff-7782-47d0-8357-2fffab96d87b")
	)
	(pad "5" smd roundrect
		(at 1.475 0.975)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_right bottom_right)
		(uuid "42e258da-077c-43c3-a1b9-f1187ed09c73")
	)
	(pad "6" smd roundrect
		(at 1.475 0.327)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_right bottom_right)
		(uuid "9ee9be5b-d88b-4192-96df-50bd42e901b8")
	)
	(pad "7" smd roundrect
		(at 1.475 -0.327)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_right bottom_right)
		(uuid "148475e6-07e1-49f5-887a-48bae360180f")
	)
	(pad "8" smd roundrect
		(at 1.475 -0.975)
		(size 0.85 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_right bottom_right)
		(uuid "4d5d2876-fb80-454b-9819-0a29e6298f36")
	)
	(pad "9" thru_hole circle
		(at -0.5 -0.75)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "6bbdfd1d-06dc-42be-ab31-f3f51ec1c457")
	)
	(pad "9" thru_hole circle
		(at -0.5 0.75)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "f43e6304-50a8-4cc2-aa34-00602052eedd")
	)
	(pad "9" thru_hole circle
		(at 0 0)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "2659db6f-15a9-4de4-85fb-4bc9a827f099")
	)
	(pad "9" smd rect
		(at 0 0)
		(size 1.65 2.4)
		(layers "F.Cu" "F.Mask")
		(uuid "6d3aaa4c-880b-461d-b87e-c641bf301694")
	)
	(pad "9" thru_hole circle
		(at 0.5 -0.75)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "09e55505-1103-4b09-8cb4-77ca56535e92")
	)
	(pad "9" thru_hole circle
		(at 0.5 0.75)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "c9a0812c-c7fa-4e76-9265-8063d5fb176e")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/VSON-8_3.3x3.3mm_P0.65mm_NexFET.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
