(footprint "Texas_VQNF_29_4x4"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3.1 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "5afe991c-2ed6-40b6-96ce-acd28e23a30c")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "Texas_VQNF_29_4x4"
		(at 0 3.2 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "63be4e20-5ee7-47a3-81e3-e09a3a3f735d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7d6da3bc-00a1-4a13-a3cb-ac90f6acd8e9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fe7ced8b-5f1b-4e43-8e7a-bd59a050875d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.05 -1.9)
		(end -1.9 -2.05)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "91f17c19-5ddf-4500-b6dc-bfa526ab1698")
	)
	(fp_line
		(start -2.05 -1.8)
		(end -2.05 -1.9)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "d3bda032-ee1b-4374-a520-56bd603e67e6")
	)
	(fp_line
		(start -2.05 2.05)
		(end -2.05 1.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "fb023855-b4e5-402e-8cc6-b1ce8321b80a")
	)
	(fp_line
		(start -2.05 2.05)
		(end -1.8 2.05)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "d93ae045-b128-4d5e-9457-6b046cd21336")
	)
	(fp_line
		(start -1.9 -2.05)
		(end -1.8 -2.05)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a3cba265-eb7c-4726-b44e-6d79323a8f38")
	)
	(fp_line
		(start 2.05 -2.05)
		(end 1.8 -2.05)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "16eae76f-321a-4a93-9250-a86ace004768")
	)
	(fp_line
		(start 2.05 -2.05)
		(end 2.05 -1.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "82ce2222-94f0-4092-8a42-0276f0464b78")
	)
	(fp_line
		(start 2.05 2.05)
		(end 1.8 2.05)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "78fdf60d-5d6e-4151-b146-2d2f1a13674f")
	)
	(fp_line
		(start 2.05 2.05)
		(end 2.05 1.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a02df33a-87fd-418f-9c5a-f3ed61384364")
	)
	(fp_rect
		(start -2.3 -2.3)
		(end 2.3 2.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "aa5f7882-f271-4003-82a1-5d1306751bb6")
	)
	(fp_text user "${REFERENCE}"
		(at 0 4.8 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "03d3a19f-8fb7-46f2-8f44-b81de37c70c4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -1.725 -1.6)
		(size 0.95 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "72127a4f-5170-4d5f-b63c-773105e85cdf")
	)
	(pad "1" smd roundrect
		(at -1.35 -1.85 90)
		(size 0.7 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "60200213-584a-4fe3-b1f9-84afb4c36b06")
	)
	(pad "2" smd roundrect
		(at -1.9 -1.2 180)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "928d1bdf-5558-4096-8901-4c4592e49dfd")
	)
	(pad "3" smd roundrect
		(at -1.9 -0.8 180)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "42abe885-85a1-4924-a011-654af210fc73")
	)
	(pad "4" smd roundrect
		(at -1.9 -0.4 180)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "ace14d3f-e69e-4a67-babf-b9c72a3241f2")
	)
	(pad "5" smd roundrect
		(at -1.9 0 180)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "1a2622a0-973f-471f-bdb9-e72926ba1de4")
	)
	(pad "6" smd roundrect
		(at -1.9 0.4 180)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "471900f1-251c-41ea-b0e8-748347f30cee")
	)
	(pad "7" smd roundrect
		(at -1.9 0.8 180)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "4739c9c4-0d94-43fd-9f03-b46749c16c8e")
	)
	(pad "8" smd roundrect
		(at -1.9 1.2 180)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "b185bf5e-fceb-48d8-bca8-0ecb49bdd059")
	)
	(pad "9" smd roundrect
		(at -1.75 1.6 180)
		(size 0.9 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "ea5ab833-c272-4580-9c13-98ee591acadc")
	)
	(pad "9" smd roundrect
		(at -1.4 1.85 270)
		(size 0.7 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "46845a8b-f109-444e-9e44-80a9c1611973")
	)
	(pad "10" smd roundrect
		(at -1 1.9 270)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "58f8073d-a266-494d-9607-d9e3b543e45a")
	)
	(pad "11" smd roundrect
		(at -0.6 1.9 270)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "23983c0a-3a31-4c54-8083-aed144b21b0d")
	)
	(pad "12" smd roundrect
		(at -0.2 1.9 270)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "3eb4238c-2139-458a-9452-a1806889add6")
	)
	(pad "13" smd roundrect
		(at 0.2 1.9 270)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "d65e0cec-028e-432c-8b48-50171473aa15")
	)
	(pad "14" smd roundrect
		(at 0.6 1.9 270)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "2918b1e8-1529-46d8-ab34-599fb83e9f9b")
	)
	(pad "15" smd roundrect
		(at 1 1.9 270)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "a0b683e0-779c-457c-ace9-ec3ebe91daaf")
	)
	(pad "16" smd roundrect
		(at 1.4 1.85 270)
		(size 0.7 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "ae29fd18-9e2b-4314-a317-f98364e756a0")
	)
	(pad "16" smd roundrect
		(at 1.75 1.6)
		(size 0.9 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "389ba6c5-9f02-44ba-bfab-21cd5758e87d")
	)
	(pad "17" smd roundrect
		(at 1.85 1.2)
		(size 0.7 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "65cf7ea2-1ec0-4d2c-907e-fe00b40e09d6")
	)
	(pad "18" smd roundrect
		(at 1.875 0.8)
		(size 0.65 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "681e501b-d560-4073-a676-6731f8a5d3db")
	)
	(pad "19" smd roundrect
		(at 1.8625 0.4)
		(size 0.68 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "0e2944cd-b6e2-4dff-a409-efcda9c39467")
	)
	(pad "20" smd roundrect
		(at 1.9 0)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "63967368-ece0-4498-b9fd-c466d5221073")
	)
	(pad "21" smd roundrect
		(at 1.9 -0.4)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "cee7e747-3aa3-4286-9375-a87a272ac394")
	)
	(pad "22" smd roundrect
		(at 1.9 -0.8)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "84a5d1cd-6b14-42db-8ffd-6b17942d2c2d")
	)
	(pad "23" smd roundrect
		(at 1.9 -1.2)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "dd0f9297-9626-4eac-a319-515770ba20c8")
	)
	(pad "24" smd roundrect
		(at 1.35 -1.85 90)
		(size 0.7 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "84b094f5-53ea-4d87-a898-9a372d957870")
	)
	(pad "24" smd roundrect
		(at 1.725 -1.6)
		(size 0.95 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "54f7fa8e-b617-4c9b-9c9e-123662bc7130")
	)
	(pad "25" smd roundrect
		(at 0.9 -1.7 90)
		(size 1 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "45282fbf-9bb7-4aa1-9adb-408c2763a9bb")
	)
	(pad "26" smd roundrect
		(at 0.45 -1.7 90)
		(size 1 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "bf6b6183-571e-4e9c-b1c8-10ea4c76836b")
	)
	(pad "27" smd roundrect
		(at 0 -1.7 90)
		(size 1 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "39c4b646-f0fe-49dc-bb65-5c0e1714bd27")
	)
	(pad "28" smd roundrect
		(at -0.45 -1.7 90)
		(size 1 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "dd2a1b9d-1b19-4a91-a5e9-c99aa404fd1e")
	)
	(pad "29" smd roundrect
		(at -0.9 -1.725 90)
		(size 0.95 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "4e1054d9-f68f-42a8-baae-9ef35ec1e418")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/WSON-8_4x4mm_P0.8mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
