(footprint "ESN4"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -2.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "7cfbc37f-4678-4ba3-8428-57b957a0fc94")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "ESN4"
		(at 0 -0.8 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "b3f537d9-bc6a-4cb1-904b-cc97d6bd2b8b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "../../../../doc/datasheets/LiIon Protection/XB4908.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "57392a18-2d0d-4687-b2a9-bbcecb3e94fc")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6bc6ac70-16dc-4f04-9243-faee36cd5070")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_poly
		(pts
			(xy -1.85 -1.65) (xy -1.45 -1.65) (xy -1.65 -1.35)
		)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "084cce54-6d9b-4eab-978f-b183c22588cf")
	)
	(fp_rect
		(start -2.15 -1.675)
		(end 2.15 1.675)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "ff77d0a4-c1cd-4cf7-a5e5-0eba6acb6670")
	)
	(fp_rect
		(start -1.15 -1.4)
		(end 1.15 1.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "e375870b-9f7b-44e0-950c-a6f973fcd63a")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0.7 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "75a216b8-c3e9-4c2e-a898-8ae4e80a6381")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -1.632 -0.793)
		(size 0.636 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "ef4f3180-156b-4edd-8e8a-407b3d466b9e")
	)
	(pad "2" smd rect
		(at -1.632 0.445)
		(size 0.636 1.146)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "ff8956fc-c762-47a6-a404-a45bb1832b93")
	)
	(pad "3" smd rect
		(at 1.632 0.5365)
		(size 0.663 0.873)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "ef49f64d-beed-49be-aa46-87820fa9d145")
	)
	(pad "4" smd rect
		(at 1.632 -0.5365)
		(size 0.636 0.873)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "af0dd650-7d84-4dff-ba2c-32a7398fd15a")
	)
	(embedded_fonts no)
	(model "../3D/ESN4.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 -0 -0)
		)
	)
)
