(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(U201-VDD)")
	(net 2 "/Power/BAT-")
	(net 3 "/Power/BAT+")
	(net 4 "Net-(U202-SRN)")
	(net 5 "GND")
	(net 6 "unconnected-(U202-V_{DD}-Pad5)")
	(net 7 "/Power/BATK-")
	(net 8 "unconnected-(U202-NC-Pad11)")
	(net 9 "unconnected-(U202-BIN-Pad10)")
	(net 10 "unconnected-(U202-NC-Pad4)")
	(net 11 "unconnected-(U202-SCL-Pad2)")
	(net 12 "/Power/BATK+")
	(net 13 "unconnected-(U202-SDA-Pad1)")
	(net 14 "unconnected-(U202-GPOUT-Pad12)")
	(net 15 "unconnected-(U202-NC-Pad9)")
	(net 16 "NTC")
	(net 17 "Net-(U202-SRP)")
	(footprint "Connector_JST:JST_GH_BM04B-GHS-TBT_1x04-1MP_P1.25mm_Vertical"
		(layer "F.Cu")
		(uuid "55b25781-057c-49bb-86db-dcd49f7b2a88")
		(at 116.475 60.2)
		(descr "JST GH series connector, BM04B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST GH vertical")
		(property "Reference" "J202"
			(at 0 -4 0)
			(layer "F.SilkS")
			(uuid "02966a91-9812-4363-8485-4a4d6de242f5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "JST GH"
			(at 0 4 0)
			(layer "F.Fab")
			(uuid "b4aac657-abc8-406e-ad84-151d0715a6e6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b0240890-f44f-40ce-a9a6-46ed463a6957")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b7c14642-d986-4fe7-8ccb-d57a67b08e1d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "JST_GH_BM04B-GHS-*_1x04-*")
		(path "/c0628d30-5a3b-4320-aa2a-0a2a91f3280a/c9bd4091-cc37-48b0-a3be-c995286d6369")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.235 0.26)
			(end -4.235 1.86)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "391f211a-c13c-4414-808c-11b3aad4e5b4")
		)
		(fp_line
			(start -4.235 1.86)
			(end -2.435 1.86)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0e3dbe32-bdf4-40e1-a98c-eef7ffa84f33")
		)
		(fp_line
			(start -2.965 -2.61)
			(end 2.965 -2.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d2234fb4-663d-4404-8bfd-7f046b5f201e")
		)
		(fp_line
			(start -2.435 1.86)
			(end -2.435 2.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "16ada4bd-479a-4637-861c-a542ee47e34e")
		)
		(fp_line
			(start 4.235 0.26)
			(end 4.235 1.86)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5f0022a4-c71f-49c4-a229-ec1b626a4e28")
		)
		(fp_line
			(start 4.235 1.86)
			(end 2.435 1.86)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cdd4fe9a-d527-4765-a98d-79c3c40b15e6")
		)
		(fp_line
			(start -4.73 -3.3)
			(end -2.72 -3.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "23cd5b07-7fa3-4a83-8289-ec6cfb6d5238")
		)
		(fp_line
			(start -4.73 0.5)
			(end -4.73 -3.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b23b41c2-4a3a-4f76-9eeb-c492f40a968b")
		)
		(fp_line
			(start -4.63 0.5)
			(end -4.73 0.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e5e91bcf-b46d-471d-937e-15509fe22bf1")
		)
		(fp_line
			(start -4.63 2.25)
			(end -4.63 0.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "792305a7-9400-49b2-a857-ac1d19daf60e")
		)
		(fp_line
			(start -2.72 -3.3)
			(end -2.72 -3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f4576917-15b9-4a5c-994a-338bbc4ea81f")
		)
		(fp_line
			(start -2.72 -3)
			(end 2.72 -3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4f21cccb-c87e-4daf-bd4a-f813fec641aa")
		)
		(fp_line
			(start -2.68 2.25)
			(end -4.63 2.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6de755d3-b665-4e8d-a626-04ec80bbfae5")
		)
		(fp_line
			(start -2.68 3.3)
			(end -2.68 2.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "408519fc-e17d-419b-8970-93dc4106d9c0")
		)
		(fp_line
			(start 2.68 2.25)
			(end 2.68 3.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fec87bbf-24d0-489f-9fd6-8845ae113a4d")
		)
		(fp_line
			(start 2.68 3.3)
			(end -2.68 3.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b87ff24c-0c6a-4b82-a6c7-c6d71a532bb6")
		)
		(fp_line
			(start 2.72 -3.3)
			(end 4.73 -3.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "749baefc-58fe-4fa5-a0e3-03652eb7bf1b")
		)
		(fp_line
			(start 2.72 -3)
			(end 2.72 -3.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b7fc1a40-3f3a-4ec1-9694-4c1986bc36af")
		)
		(fp_line
			(start 4.63 0.5)
			(end 4.63 2.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "50257ac7-97f1-470a-b009-5fa717490ac2")
		)
		(fp_line
			(start 4.63 2.25)
			(end 2.68 2.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "14a09442-f31e-434c-8d48-c7222ce300f7")
		)
		(fp_line
			(start 4.73 -3.3)
			(end 4.73 0.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fcc13bac-ea8a-47be-8f36-2637ba7dc6e5")
		)
		(fp_line
			(start 4.73 0.5)
			(end 4.63 0.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c93f03eb-03c5-44e1-aa38-22fa01132f04")
		)
		(fp_line
			(start -4.125 -2.5)
			(end 4.125 -2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b4594aae-4215-4b7c-a8c8-5a66c0a8c351")
		)
		(fp_line
			(start -4.125 1.75)
			(end -4.125 -2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b2349891-89ac-4bde-a314-cc581e9d9e35")
		)
		(fp_line
			(start -4.125 1.75)
			(end 4.125 1.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eaefc7e4-4889-4967-b16f-f64d0525c0ab")
		)
		(fp_line
			(start -2.375 1.75)
			(end -1.875 1.042893)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5bc1a3b0-4da7-4f46-8947-b2401d252eff")
		)
		(fp_line
			(start -1.875 1.042893)
			(end -1.375 1.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "143afc98-a74a-422e-a322-5d0345f003d5")
		)
		(fp_line
			(start 4.125 1.75)
			(end 4.125 -2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ab594b81-9a21-4fe7-8313-50cc5d3f93c9")
		)
		(fp_rect
			(start -2.125 -0.5)
			(end -1.625 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "b8367b40-dcec-4ebc-9b9a-9b5f59cdfd96")
		)
		(fp_rect
			(start -0.875 -0.5)
			(end -0.375 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "9238478e-0b2a-41c1-abd4-97485f1a23d3")
		)
		(fp_rect
			(start 0.375 -0.5)
			(end 0.875 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "b38dabd5-b902-4106-9949-9e03883b84ee")
		)
		(fp_rect
			(start 1.625 -0.5)
			(end 2.125 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "f32084c4-7f1b-4ea4-8a60-8ef9a4606183")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 0)
			(layer "F.Fab")
			(uuid "649a66b8-9c26-4f0d-82f1-20da76ae1a33")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.875 1.95)
			(size 0.6 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "/Power/BATK+")
			(pintype "passive")
			(uuid "acd12daf-6bbc-41c7-b42f-536bec56fc2c")
		)
		(pad "2" smd roundrect
			(at -0.625 1.95)
			(size 0.6 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "NTC")
			(pintype "passive")
			(uuid "803361b3-67a2-4cf8-a444-8d6a936ac9bf")
		)
		(pad "3" smd roundrect
			(at 0.625 1.95)
			(size 0.6 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "GND")
			(pintype "passive")
			(uuid "8b02aa49-c035-4f09-9be9-666cc392f433")
		)
		(pad "4" smd roundrect
			(at 1.875 1.95)
			(size 0.6 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/Power/BATK-")
			(pintype "passive")
			(uuid "8af0e95e-d9b1-4f2a-911d-f7bda0ae12da")
		)
		(pad "MP" smd roundrect
			(at -3.725 -1.4)
			(size 1 2.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/Power/BATK-")
			(pintype "passive")
			(uuid "c6b7fac4-05cb-40de-a4c4-d8eae256a014")
		)
		(pad "MP" smd roundrect
			(at 3.725 -1.4)
			(size 1 2.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/Power/BATK-")
			(pintype "passive")
			(uuid "3ae17c05-d5ef-4e36-9b1e-a7f0d28f8ead")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_GH_BM04B-GHS-TBT_1x04-1MP_P1.25mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PowerProfiler:ESN4"
		(layer "F.Cu")
		(uuid "6ceb05b3-b721-423e-86b3-fd456ed2ebc5")
		(at 131.345 73.707 -90)
		(property "Reference" "U201"
			(at 0 -2.5 270)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "9c078233-3117-4d13-8816-9b47b7c95984")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "XB4908"
			(at 0 -0.8 270)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "6b54eadc-4f4c-4469-ad48-006fd725652a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "kicad-embed://XB4908.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ff5d26dd-a143-4011-af2d-b79e26367b40")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "One Cell Lithium-ion/Polymer Battery Protection IC"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0767fee4-0b14-45cb-95f5-1b28743d938e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/c0628d30-5a3b-4320-aa2a-0a2a91f3280a/2e2b7c36-a080-4f60-b353-1c18952e027e")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_poly
			(pts
				(xy -1.85 -1.65) (xy -1.45 -1.65) (xy -1.65 -1.35)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "110f6c10-b0b8-4a41-ac71-ac5308327796")
		)
		(fp_rect
			(start -2.15 -1.675)
			(end 2.15 1.675)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "eb666b0f-0d89-4938-ac83-db87dd0c0fc5")
		)
		(fp_rect
			(start -1.15 -1.4)
			(end 1.15 1.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "8b8efc5b-411a-4616-848b-f74df3a76a44")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0.7 270)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "6306f493-79b2-43e3-8264-c8794d28f06c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at -1.632 -0.793 270)
			(size 0.636 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(U201-VDD)")
			(pinfunction "VDD")
			(pintype "power_in")
			(uuid "9c505cad-20e9-45f8-a0ff-0f7beac0c54e")
		)
		(pad "2" smd rect
			(at -1.632 0.445 270)
			(size 0.636 1.146)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/Power/BAT-")
			(pinfunction "BAT-")
			(pintype "power_in")
			(uuid "62de68f8-ee4a-416e-aca8-44b2d6e7458c")
		)
		(pad "3" smd rect
			(at 1.632 0.5365 270)
			(size 0.663 0.873)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "GND")
			(pinfunction "PACK-")
			(pintype "power_out")
			(uuid "8a3a1332-6cc1-455e-aca8-6841894e0a1c")
		)
		(pad "4" smd rect
			(at 1.632 -0.5365 270)
			(size 0.636 0.873)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "GND")
			(pinfunction "PACK-")
			(pintype "input")
			(uuid "501e9cd9-5af1-4635-98fc-c5f22f609797")
		)
		(embedded_fonts no)
		(model "../3D/ESN4.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(uuid "728dfc53-f8e3-477b-b936-1715a43c444b")
		(at 131.38 71.075 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C201"
			(at 0 -1.16 0)
			(layer "F.SilkS")
			(uuid "8dfbdee0-477a-43bb-95b1-6fbbfcd8b78d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100n"
			(at 0 1.16 0)
			(layer "F.Fab")
			(uuid "53d4249b-56cd-4d05-ba12-287902351cc1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "02476dd2-98f6-44aa-b62c-d0c67ce11834")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "93b65ab0-4c9d-4582-b669-67326c3f37dd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/c0628d30-5a3b-4320-aa2a-0a2a91f3280a/e0c0274c-0f2a-4627-b046-b387329d08be")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.107836 0.36)
			(end 0.107836 0.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "446703b6-d5a7-49e8-b0b5-ef2944432d73")
		)
		(fp_line
			(start -0.107836 -0.36)
			(end 0.107836 -0.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "508c7b81-fcad-4916-b8a7-dee6f0e01dac")
		)
		(fp_line
			(start 0.91 0.46)
			(end -0.91 0.46)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "12c7ca08-3643-422d-8ac6-3ccfc99f5ebc")
		)
		(fp_line
			(start 0.91 -0.46)
			(end 0.91 0.46)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d1fe5049-b2cd-4595-a123-3e4cc8a998f7")
		)
		(fp_line
			(start -0.91 0.46)
			(end -0.91 -0.46)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "abc9726f-a8a2-4f5f-997e-dde3a4e6aa14")
		)
		(fp_line
			(start -0.91 -0.46)
			(end 0.91 -0.46)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3a4b927d-eb66-4340-a540-2e104401fa06")
		)
		(fp_line
			(start 0.5 0.25)
			(end -0.5 0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4bb97356-0346-4971-be28-06aa50d1afce")
		)
		(fp_line
			(start 0.5 -0.25)
			(end 0.5 0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fa4c8711-96e7-4f21-8c70-0f4e2da22420")
		)
		(fp_line
			(start -0.5 0.25)
			(end -0.5 -0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "412f2d38-e002-4ad5-8637-cb584e764c6a")
		)
		(fp_line
			(start -0.5 -0.25)
			(end 0.5 -0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c912719e-0981-484f-a895-35f1d8a43eba")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "45b1e6c0-f422-443d-97a9-80b8465cb121")
			(effects
				(font
					(size 0.25 0.25)
					(thickness 0.04)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(U201-VDD)")
			(pintype "passive")
			(uuid "cb2599ce-1c54-4c32-b1db-5f75d1f2f152")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/Power/BAT-")
			(pintype "passive")
			(uuid "799a4e29-dfde-4385-bb57-11deddd5c500")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SON:Texas_S-PDSO-N12"
		(layer "F.Cu")
		(uuid "928e37bc-b7d8-4015-b900-cd8dcb1334d2")
		(at 117.4 69.6)
		(descr "http://www.ti.com/lit/ds/symlink/bq27441-g1.pdf")
		(tags "SON thermal pads")
		(property "Reference" "U202"
			(at -0.000701 -2.517393 0)
			(layer "F.SilkS")
			(uuid "b146abc3-d741-4873-a824-e4589adce7f1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BQ27441-G1"
			(at -0.000701 2.852607 0)
			(layer "F.Fab")
			(uuid "9d0a2668-a2c6-4176-9b7b-79ddc90da833")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq27441-g1.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8873fb86-2584-4788-b7d8-2f8837ca599b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "System Side Li Ion/Polymer Fuel Gauge, PDSON-12"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5ccea781-45db-4867-8ad1-ce8c96c29c1f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*PDSO*N12*")
		(path "/c0628d30-5a3b-4320-aa2a-0a2a91f3280a/94229e19-5a59-4174-a445-95d84c88c3c4")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.56 -1.397393)
			(end -1.93 -1.397393)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cf149ac4-7b97-4abc-a68d-8f8474800b94")
		)
		(fp_line
			(start -1.56 1.4)
			(end -2.1 1.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9fb800ef-0b0c-4935-8438-f28939c4504d")
		)
		(fp_line
			(start 0.64 -1.4)
			(end -0.64 -1.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e2f5e2bb-6d22-434b-b83b-00d2be02ede2")
		)
		(fp_line
			(start 0.64 1.4)
			(end -0.64 1.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8c72cf11-63d8-42da-b42b-e28e575e6259")
		)
		(fp_line
			(start 1.56 -1.4)
			(end 2.1 -1.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cf209290-2a18-4fe4-b17b-fea6b711478f")
		)
		(fp_line
			(start 1.56 1.4)
			(end 2.1 1.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5bb0f32e-fb6a-4975-9696-015a05e054c0")
		)
		(fp_poly
			(pts
				(xy -2.26 -1.4) (xy -2.5 -1.73) (xy -2.02 -1.73) (xy -2.26 -1.4)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "178ba6f1-f5ac-482a-b020-7fef7a10767d")
		)
		(fp_rect
			(start -2.45 -1.7)
			(end 2.45 1.7)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "2b8cd6c0-fa96-4fa3-8bd8-443b0c77640d")
		)
		(fp_line
			(start -2 -0.5)
			(end -2 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "742e8991-a6fa-45d3-88cb-c696cd866429")
		)
		(fp_line
			(start -2 -0.5)
			(end -1.25 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "090d110f-dd74-4637-bab4-bf005c6de122")
		)
		(fp_line
			(start -2 1.25)
			(end 2 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "88af3a5f-6472-4bf2-b4d6-c78c1928b33a")
		)
		(fp_line
			(start -1.25 -1.25)
			(end 2 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5ce6a54b-44a9-4b0a-9358-1ee8d50e140d")
		)
		(fp_line
			(start 2 1.25)
			(end 2 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fc38d913-25a6-4617-9dcb-c212c8e243c3")
		)
		(fp_text user "${REFERENCE}"
			(at -0.000701 0.002607 0)
			(layer "F.Fab")
			(uuid "0135b957-13e1-40a2-b6d9-49803afc290c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" smd roundrect
			(at -1.125 -1.2625)
			(size 0.2 0.375)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "f4d37a9f-dca5-4337-8046-f3cbc7999b25")
		)
		(pad "" smd roundrect
			(at -1.125 1.2625)
			(size 0.2 0.375)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "13bc8ae5-1ff5-4b3a-84f0-b1b7e4b42801")
		)
		(pad "" smd roundrect
			(at -0.64 0)
			(size 1.08 1.75)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "b2fcdc05-284e-4605-88ba-5e986526f3ab")
		)
		(pad "" smd roundrect
			(at 0.64 0)
			(size 1.08 1.75)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "e36a24f5-a4ba-427f-9534-6099b1938335")
		)
		(pad "" smd roundrect
			(at 1.125 -1.2625)
			(size 0.2 0.375)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "c41cf989-1b3e-465a-a157-a3079376564d")
		)
		(pad "" smd roundrect
			(at 1.125 1.2625)
			(size 0.2 0.375)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "9488c678-7444-41f1-9e5b-f6495c6eec18")
		)
		(pad "1" smd roundrect
			(at -1.9 -1)
			(size 0.6 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2)
			(chamfer)
			(net 13 "unconnected-(U202-SDA-Pad1)")
			(pinfunction "SDA")
			(pintype "bidirectional")
			(uuid "d40826ea-b1da-4e6f-9d08-5a8f0744830b")
		)
		(pad "2" smd roundrect
			(at -1.9 -0.6)
			(size 0.6 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2)
			(chamfer)
			(net 11 "unconnected-(U202-SCL-Pad2)")
			(pinfunction "SCL")
			(pintype "input")
			(uuid "ab9f2186-9f92-4b1d-b8f7-a05491b0b1c5")
		)
		(pad "3" smd roundrect
			(at -1.9 -0.2)
			(size 0.6 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2)
			(chamfer)
			(net 7 "/Power/BATK-")
			(pinfunction "V_{SS}")
			(pintype "power_in")
			(uuid "383ab41e-1b0e-4aee-80b6-df7c70f61e6e")
		)
		(pad "4" smd roundrect
			(at -1.9 0.2)
			(size 0.6 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2)
			(chamfer)
			(net 10 "unconnected-(U202-NC-Pad4)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "5a0f55ec-0942-43ab-b72e-9cfd0910a19d")
		)
		(pad "5" smd roundrect
			(at -1.9 0.6)
			(size 0.6 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2)
			(chamfer)
			(net 6 "unconnected-(U202-V_{DD}-Pad5)")
			(pinfunction "V_{DD}")
			(pintype "power_out")
			(uuid "031e7391-526f-4323-841e-2a35b664d031")
		)
		(pad "6" smd roundrect
			(at -1.9 1)
			(size 0.6 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2)
			(chamfer)
			(net 12 "/Power/BATK+")
			(pinfunction "BAT")
			(pintype "power_in")
			(uuid "ce43cbc5-629c-4a3e-b9cf-1bcc28fb33bc")
		)
		(pad "7" smd roundrect
			(at 1.9 1)
			(size 0.6 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2)
			(chamfer)
			(net 4 "Net-(U202-SRN)")
			(pinfunction "SRN")
			(pintype "input")
			(uuid "516fae61-ca96-4df0-a703-0cfdc5504d70")
		)
		(pad "8" smd roundrect
			(at 1.9 0.6)
			(size 0.6 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2)
			(chamfer)
			(net 17 "Net-(U202-SRP)")
			(pinfunction "SRP")
			(pintype "input")
			(uuid "445d83f0-87e3-46dc-90a8-d69a9f5b8f84")
		)
		(pad "9" smd roundrect
			(at 1.9 0.2)
			(size 0.6 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2)
			(chamfer)
			(net 15 "unconnected-(U202-NC-Pad9)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "f083ba98-25c6-471d-a1be-3a5e1b89c3eb")
		)
		(pad "10" smd roundrect
			(at 1.9 -0.2)
			(size 0.6 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2)
			(chamfer)
			(net 9 "unconnected-(U202-BIN-Pad10)")
			(pinfunction "BIN")
			(pintype "input")
			(uuid "52e90c5b-4848-49f0-ab17-6bb597ae85c9")
		)
		(pad "11" smd roundrect
			(at 1.9 -0.6)
			(size 0.6 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2)
			(chamfer)
			(net 8 "unconnected-(U202-NC-Pad11)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "1f6d21e4-5277-4929-853a-a149aaf0f94f")
		)
		(pad "12" smd roundrect
			(at 1.9 -1)
			(size 0.6 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2)
			(chamfer)
			(net 14 "unconnected-(U202-GPOUT-Pad12)")
			(pinfunction "GPOUT")
			(pintype "output")
			(uuid "dd01aff5-884e-407f-b8c0-8760ae09ca1f")
		)
		(pad "13" smd roundrect
			(at -1.125 -1.1875 270)
			(size 0.525 0.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/Power/BATK-")
			(pinfunction "PAD")
			(pintype "power_in")
			(uuid "3d9a3d6d-c059-4974-abbb-dd874d76623c")
		)
		(pad "13" smd roundrect
			(at -1.125 1.1875 270)
			(size 0.525 0.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/Power/BATK-")
			(pinfunction "PAD")
			(pintype "power_in")
			(uuid "6f57dd4b-9780-4f53-9cfc-bfaf4173670b")
		)
		(pad "13" thru_hole circle
			(at -0.975 0)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 7 "/Power/BATK-")
			(pinfunction "PAD")
			(pintype "power_in")
			(uuid "a8e6dccc-f215-4c0d-8dd8-938a6ee9cc53")
		)
		(pad "13" thru_hole circle
			(at 0 -0.725)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 7 "/Power/BATK-")
			(pinfunction "PAD")
			(pintype "power_in")
			(uuid "ae8a30c9-980a-4719-8bf2-d563eb400040")
		)
		(pad "13" thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 7 "/Power/BATK-")
			(pinfunction "PAD")
			(pintype "power_in")
			(uuid "fa2f187b-6193-4698-a5b8-378dae61e398")
		)
		(pad "13" smd rect
			(at 0 0 270)
			(size 1.95 2.45)
			(layers "F.Cu" "F.Mask")
			(net 7 "/Power/BATK-")
			(pinfunction "PAD")
			(pintype "power_in")
			(uuid "4e1c3087-8cfa-40d2-bc7a-606057fdfe70")
		)
		(pad "13" thru_hole circle
			(at 0 0.725)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 7 "/Power/BATK-")
			(pinfunction "PAD")
			(pintype "power_in")
			(uuid "e0686355-b3d2-4ee6-b4bb-65fc49b9851b")
		)
		(pad "13" thru_hole circle
			(at 0.975 0)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 7 "/Power/BATK-")
			(pinfunction "PAD")
			(pintype "power_in")
			(uuid "5a88c990-254f-4179-b410-1d397a100fbc")
		)
		(pad "13" smd roundrect
			(at 1.125 -1.1875 270)
			(size 0.525 0.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/Power/BATK-")
			(pinfunction "PAD")
			(pintype "power_in")
			(uuid "1c669e72-bfe1-43b5-a1b6-7d2b3e15560e")
		)
		(pad "13" smd roundrect
			(at 1.125 1.1875 270)
			(size 0.525 0.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/Power/BATK-")
			(pinfunction "PAD")
			(pintype "power_in")
			(uuid "97afc0dd-7cf5-4bd7-94b7-65f54347b9ff")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/Texas_S-PDSO-N12.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_AMASS:AMASS_XT30PW-M_1x02_P2.50mm_Horizontal"
		(layer "F.Cu")
		(uuid "99046d33-93d1-4554-9d43-969061b27fd4")
		(at 130.9 68.275)
		(descr "Connector XT30 Horizontal PCB Male, https://www.tme.eu/Document/6eb2005a51a52592b3f19e8a450c54c8/XT30PW-M.pdf")
		(tags "RC Connector XT30")
		(property "Reference" "J201"
			(at -2.5 -14.5 0)
			(layer "F.SilkS")
			(uuid "4b5abe05-3055-45f3-aef9-863a5d46ca8a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "XT30"
			(at -2.5 3.5 0)
			(layer "F.Fab")
			(uuid "8bae02a4-560f-4378-8ada-d41510029bd1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b3cf1469-63a7-42a3-8e02-4a30f5472291")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a1a36b77-cb4a-4419-a300-a2ac17676ddd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/c0628d30-5a3b-4320-aa2a-0a2a91f3280a/b082077c-99bd-40d5-b35a-02995ca74113")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -8.15 -11.11)
			(end -7.56 -11.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a7fec0dc-ddbb-49f7-b3bc-4e78c3e8eb73")
		)
		(fp_line
			(start -8.15 -8.89)
			(end -7.56 -8.89)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a5d945d7-96b9-4fe6-ac88-cc541daa39bb")
		)
		(fp_line
			(start -7.56 -13.21)
			(end -7.56 -11.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "425792eb-5614-4489-9227-23f6eb120636")
		)
		(fp_line
			(start -7.56 -13.21)
			(end 2.56 -13.21)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ef18d625-0990-4c2d-b2ef-3408d62a0f05")
		)
		(fp_line
			(start -7.56 -8.89)
			(end -7.56 -3.99)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "66d5e114-1541-44bf-babb-90757d0fba65")
		)
		(fp_line
			(start -7.56 -3.99)
			(end 2.56 -3.99)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "683a0d34-f411-4542-b7d5-d84c4e43d55a")
		)
		(fp_line
			(start 2.56 -13.21)
			(end 2.56 -11.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4aace61e-c523-426c-9462-dbcb1ff4d281")
		)
		(fp_line
			(start 2.56 -11.11)
			(end 3.15 -11.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "540d354e-3a2a-47e2-9c23-159a9d184706")
		)
		(fp_line
			(start 2.56 -8.89)
			(end 2.56 -3.99)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "82448565-1065-4cb0-9a1c-62ba58b5196a")
		)
		(fp_line
			(start 2.56 -8.89)
			(end 3.15 -8.89)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4572aea2-0327-4b22-b258-3b4509b32510")
		)
		(fp_arc
			(start -8.15 -8.89)
			(mid -9.26 -10)
			(end -8.15 -11.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "387b146a-0ec7-466e-9099-6d0748b61d98")
		)
		(fp_arc
			(start 3.15 -11.11)
			(mid 4.26 -10)
			(end 3.15 -8.89)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b51ea81e-de6b-478f-8264-aa5ead6cf493")
		)
		(fp_line
			(start -9.65 -13.6)
			(end -9.65 2.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0b48a17d-bb16-4402-936d-898bdd85c697")
		)
		(fp_line
			(start -9.65 -13.6)
			(end 4.65 -13.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "369acacf-53b8-4cb6-b684-17ac4c98e71a")
		)
		(fp_line
			(start -9.65 2.25)
			(end 4.65 2.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4918d90e-6db8-44a4-93b4-19d8467ff53a")
		)
		(fp_line
			(start 4.65 -13.6)
			(end 4.65 2.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "64edf81d-d421-45f7-b6d8-e02d408aa592")
		)
		(fp_line
			(start -8.15 -11)
			(end -7.45 -11)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ee0ef96e-3b71-488f-b9d5-195c421d0fee")
		)
		(fp_line
			(start -8.15 -9)
			(end -7.45 -9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a73c8f57-d21c-49cb-b873-d89368de254c")
		)
		(fp_line
			(start -7.45 -13.1)
			(end -7.45 -11)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c43982e3-ca1a-462b-b694-2e54666b47ad")
		)
		(fp_line
			(start -7.45 -13.1)
			(end 2.45 -13.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "63c43d1d-e268-4a6d-ac69-a11f0e69a257")
		)
		(fp_line
			(start -7.45 -9)
			(end -7.45 -4.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2583bbd4-4dc3-4fe0-a231-3da0dd713799")
		)
		(fp_line
			(start -7.45 -4.1)
			(end 2.45 -4.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fe9fb7c5-d078-4635-ba2c-fec88a3946e7")
		)
		(fp_line
			(start 2.45 -13.1)
			(end 2.45 -11)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e3674311-c6d5-426a-809a-1cc99e7404bf")
		)
		(fp_line
			(start 2.45 -11)
			(end 3.15 -11)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "844e1a14-0e32-4cc1-8349-6ce7fa061e0f")
		)
		(fp_line
			(start 2.45 -9)
			(end 2.45 -4.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d8698492-9ef2-433f-ad52-c663b14293a8")
		)
		(fp_line
			(start 2.45 -9)
			(end 3.15 -9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "224ffd0d-b599-43d7-b749-8fa9d8122fa1")
		)
		(fp_arc
			(start -8.15 -9)
			(mid -9.15 -10)
			(end -8.15 -11)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9abc1fd2-fbf2-4181-b0c8-9035d0197d21")
		)
		(fp_arc
			(start 3.15 -11)
			(mid 4.15 -10)
			(end 3.15 -9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8274ea29-9b8b-458a-a7da-3d0346c8f684")
		)
		(fp_text user "+"
			(at -8 0 0)
			(layer "F.SilkS")
			(uuid "be68fe5e-da8a-4624-8303-6a825cbd685a")
			(effects
				(font
					(size 1.5 1.5)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "-"
			(at 3 0 0)
			(layer "F.SilkS")
			(uuid "e8235929-96d9-4ab5-9824-68f974fb1672")
			(effects
				(font
					(size 1.5 1.5)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "${REFERENCE}"
			(at -2.5 -3 0)
			(layer "F.Fab")
			(uuid "b0d16c50-b7cf-43d2-a9cb-68ef53d67a18")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" thru_hole circle
			(at -8 -10)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(uuid "42604b3d-cc04-4b51-b2fd-326fa7509b59")
		)
		(pad "" thru_hole circle
			(at 3 -10)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(uuid "37989f85-fff2-4d21-bf0b-a0be65c754c9")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 3.5 3.5)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.22)
			(net 2 "/Power/BAT-")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "7727d74c-4943-4d4a-b090-ead4696936c1")
		)
		(pad "2" thru_hole circle
			(at -5 0)
			(size 3.5 3.5)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/Power/BAT+")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "4dfacea9-ee6c-4967-927a-46af1f0505be")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_AMASS.3dshapes/AMASS_XT30PW-M_1x02_P2.50mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "lib/3D/Amass_XT30PW-M_pcb solder.stp"
			(offset
				(xyz -2.5 4 2.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -180)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(uuid "cd735c98-f60f-4d4e-9add-cdfa8e3b04d3")
		(at 133.41 71.075 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R201"
			(at 0 -1.17 0)
			(layer "F.SilkS")
			(uuid "de4d1429-ac6c-49a3-950a-f11baf5981f4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1k"
			(at 0 1.17 0)
			(layer "F.Fab")
			(uuid "80811660-d0b3-41e3-867f-b020af82e453")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2cb52dca-aeac-4c03-91bf-94400aefdfcf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3d616e0d-07b1-48e3-8835-3589f20941b4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/c0628d30-5a3b-4320-aa2a-0a2a91f3280a/979b46e6-7c89-4cb6-9d95-09f54eceb61f")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.153641 0.38)
			(end 0.153641 0.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "586535c7-946b-4b6c-a70e-cd03a8b5d4c0")
		)
		(fp_line
			(start -0.153641 -0.38)
			(end 0.153641 -0.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4efafcb6-5741-45d7-883e-c891386dc64a")
		)
		(fp_line
			(start 0.93 0.47)
			(end -0.93 0.47)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4a73a64b-fd08-462e-8d91-877cc81e978a")
		)
		(fp_line
			(start 0.93 -0.47)
			(end 0.93 0.47)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "44b7a805-f187-40b4-8339-10d5e16f767b")
		)
		(fp_line
			(start -0.93 0.47)
			(end -0.93 -0.47)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b2096f4e-89c8-495b-b663-3f6db1c68f29")
		)
		(fp_line
			(start -0.93 -0.47)
			(end 0.93 -0.47)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c6f4fac0-180e-4480-9917-ce3268c2a3ea")
		)
		(fp_line
			(start 0.525 0.27)
			(end -0.525 0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ecf96440-9d28-476e-bf72-b64ab041abb9")
		)
		(fp_line
			(start 0.525 -0.27)
			(end 0.525 0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9588eaf0-52d2-457f-b0c3-7c6b709dc2ca")
		)
		(fp_line
			(start -0.525 0.27)
			(end -0.525 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3020ae11-e137-42ae-8ed4-ecccdcb91ae7")
		)
		(fp_line
			(start -0.525 -0.27)
			(end 0.525 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ffbadb74-6dd9-40fe-b100-f4e3201a9487")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "eea4c6bb-d706-447a-968e-8046184acb3d")
			(effects
				(font
					(size 0.26 0.26)
					(thickness 0.04)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/Power/BAT+")
			(pintype "passive")
			(uuid "78588bb7-8e0e-46f8-98d2-26338b6bb838")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(U201-VDD)")
			(pintype "passive")
			(uuid "a8c89366-894c-442d-aab9-abf013367813")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 110.6 56.8)
		(end 184.6 113.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "Edge.Cuts")
		(uuid "4d3c7bb1-d7d4-46c5-b2af-5a96cb2467c0")
	)
	(embedded_fonts no)
)
