(footprint "HeatSink_9x9x5"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "580ad602-7d9a-4b5f-8625-5ec97a8b779f")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "HeatSink_9x9x5"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "dd5edd79-c9a4-4ed2-a880-eb827c1b7258")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9a04b339-c416-45bb-baca-485b4dc79590")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d2b70db2-9037-4ef8-bd91-e244a12bc3d6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_line
		(start -4.75 -4.75)
		(end -4.75 -3.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "287b1eb1-2921-4e07-8bc1-25e8cff6019f")
	)
	(fp_line
		(start -4.75 -4.75)
		(end -3.75 -4.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "496b2af4-f61e-49cf-b6d7-79908034c102")
	)
	(fp_line
		(start -4.75 4.8)
		(end -4.75 3.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "003ca7fa-12b8-457c-b065-ee040d766db5")
	)
	(fp_line
		(start -4.75 4.8)
		(end -3.75 4.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "dee913de-aa72-4074-85bb-f3a76c6bebcd")
	)
	(fp_line
		(start 4.8 -4.75)
		(end 3.8 -4.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "40186396-9aed-480e-b19b-f1c0806a268c")
	)
	(fp_line
		(start 4.8 -4.75)
		(end 4.8 -3.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "df54e04d-24ee-4fd4-baeb-072e6001bb33")
	)
	(fp_line
		(start 4.8 4.8)
		(end 3.8 4.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "1dbf9030-2d10-4b85-ab74-9419e9be9c45")
	)
	(fp_line
		(start 4.8 4.8)
		(end 4.8 3.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "0ac021e1-6393-4190-8be9-b2eff2c13c9a")
	)
	(fp_rect
		(start -4.75 -4.75)
		(end 4.8 4.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "274daba3-a744-483c-a95f-622c7f8ab708")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/3d/9x9x5.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 -0 -0)
		)
	)
)
