(footprint "DFN2x5_6L_EP1_P"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -2.1 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "44a0d549-1101-4d5b-ba2a-1266b607f3e3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "DFN2x5_6L_EP1_P"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "33b8d5c8-362e-4633-ba5d-21d5cca6502a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "822b0afe-f77f-43a2-b897-5557e49ebc2b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "979c2977-32fb-47d1-8e02-ee9d1ad7f631")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -1.385 -0.9)
		(end -0.9 0.9)
		(stroke
			(width 0)
			(type solid)
		)
		(fill yes)
		(layer "F.Mask")
		(uuid "3f372a89-6b8b-4290-8e6e-37757aa97f79")
	)
	(fp_rect
		(start -0.9 -0.9)
		(end 0.9 -0.7)
		(stroke
			(width 0)
			(type solid)
		)
		(fill yes)
		(layer "F.Mask")
		(uuid "437c4fe3-3b65-4498-8cbb-3092b20dea95")
	)
	(fp_rect
		(start -0.9 -0.3)
		(end 0.9 0.3)
		(stroke
			(width 0)
			(type solid)
		)
		(fill yes)
		(layer "F.Mask")
		(uuid "17c54e19-eefb-4cb4-8a30-22769fa63e22")
	)
	(fp_rect
		(start -0.9 0.7)
		(end 0.9 0.9)
		(stroke
			(width 0)
			(type solid)
		)
		(fill yes)
		(layer "F.Mask")
		(uuid "8c091947-de48-4bc0-8baa-99cee4714fca")
	)
	(fp_rect
		(start -0.5 -0.9)
		(end 0.5 0.9)
		(stroke
			(width 0)
			(type solid)
		)
		(fill yes)
		(layer "F.Mask")
		(uuid "cf3122f2-1410-4ffa-bd3a-95e240a42250")
	)
	(fp_rect
		(start 1.385 -0.9)
		(end 0.9 0.9)
		(stroke
			(width 0)
			(type solid)
		)
		(fill yes)
		(layer "F.Mask")
		(uuid "ebc6d5a1-7eef-4f5f-8baa-09a348a60ff0")
	)
	(fp_circle
		(center -0.7 -0.5)
		(end -0.45 -0.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Mask")
		(uuid "52574f56-bb94-4404-98ae-8acf527bf158")
	)
	(fp_circle
		(center -0.7 0.5)
		(end -0.45 0.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Mask")
		(uuid "ff337c18-50c8-4182-803e-34fcf5daaf88")
	)
	(fp_circle
		(center 0.7 -0.5)
		(end 0.95 -0.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Mask")
		(uuid "fd631b03-8a39-494f-92a6-7640a9c66c59")
	)
	(fp_circle
		(center 0.7 0.5)
		(end 0.95 0.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Mask")
		(uuid "98ae19ae-30e7-445d-8be0-9b34eabae267")
	)
	(fp_line
		(start -2.3 1.05)
		(end -2.3 0.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "42bf5688-e4a9-45a1-ad36-429bed749752")
	)
	(fp_line
		(start -2.3 1.05)
		(end 2.3 1.05)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "104eef33-86b8-4489-9056-9edb6bd92178")
	)
	(fp_line
		(start -1.85 -1.05)
		(end 2.3 -1.05)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ba0659d8-b83b-46ae-b3d3-402c6ef27017")
	)
	(fp_line
		(start 2.3 -1.05)
		(end 2.3 -0.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "921d3a9b-7420-48e0-a47f-cfcbaca36335")
	)
	(fp_line
		(start 2.3 1.05)
		(end 2.3 0.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "43b816cc-cfff-4d90-9de0-d61ec583d3fd")
	)
	(fp_poly
		(pts
			(xy -2.45 -0.8) (xy -2.55 -0.95) (xy -2.35 -0.95)
		)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "c4927c74-802e-4214-806a-02e285ebbf56")
	)
	(fp_rect
		(start -1.385 -0.9)
		(end -0.9 0.9)
		(stroke
			(width 0)
			(type solid)
		)
		(fill yes)
		(layer "F.Paste")
		(uuid "2b773e10-eb6f-449f-8e04-9c9c33bdbbf9")
	)
	(fp_rect
		(start -0.9 -0.3)
		(end 0.9 0.3)
		(stroke
			(width 0)
			(type solid)
		)
		(fill yes)
		(layer "F.Paste")
		(uuid "989bde29-a11b-4306-9c5b-e0ac37b279b6")
	)
	(fp_rect
		(start -0.5 -0.9)
		(end 0.5 0.9)
		(stroke
			(width 0)
			(type solid)
		)
		(fill yes)
		(layer "F.Paste")
		(uuid "d5e02262-62b7-412b-8b32-c21825bb6caa")
	)
	(fp_rect
		(start 1.385 -0.9)
		(end 0.9 0.9)
		(stroke
			(width 0)
			(type solid)
		)
		(fill yes)
		(layer "F.Paste")
		(uuid "38ed4447-2b66-4a63-a6a9-82e261650bc2")
	)
	(fp_rect
		(start -2.6 -1.1)
		(end 2.6 1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "ec5bfc4d-edf6-40b0-8061-df21c3f33ca1")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "85408de3-96a7-4e1d-9389-0fd0794572a5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -2.255 -0.5)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "481f2b4d-c19e-46a0-a36c-65c16997edf3")
	)
	(pad "2" smd rect
		(at -2.255 0)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "3688eeed-5456-4dd5-9dcb-3ba46f0c9afa")
	)
	(pad "3" smd rect
		(at -2.255 0.5)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "33e39039-6c7b-4fe9-b007-3f5c1bfccc72")
	)
	(pad "4" smd rect
		(at 2.255 0.5)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "e2c8e7b4-7bc3-499f-b71c-59a69e9fed6a")
	)
	(pad "5" smd rect
		(at 2.255 0)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "fc806946-3c8b-4b95-bf35-f25535f24917")
	)
	(pad "6" smd rect
		(at 2.255 -0.5)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "6820b794-3cf0-4818-9a4a-2d9bb7babb63")
	)
	(pad "7" thru_hole circle
		(at -0.7 -0.5)
		(size 0.4 0.4)
		(drill 0.2)
		(layers "*.Cu" "B.Mask")
		(remove_unused_layers no)
		(uuid "614344d8-37d7-4e8e-a378-4a3971630a98")
	)
	(pad "7" thru_hole circle
		(at -0.7 0.5)
		(size 0.4 0.4)
		(drill 0.2)
		(layers "*.Cu" "B.Mask")
		(remove_unused_layers no)
		(uuid "195a91f6-13e1-4c7b-9754-0f95ecbe9a21")
	)
	(pad "7" smd rect
		(at 0 0)
		(size 2.77 1.8)
		(layers "F.Cu")
		(uuid "fb2847c7-0901-4ae1-8936-39546a6fdbaf")
	)
	(pad "7" thru_hole circle
		(at 0.7 -0.5)
		(size 0.4 0.4)
		(drill 0.2)
		(layers "*.Cu" "B.Mask")
		(remove_unused_layers no)
		(uuid "607aea58-68a7-4a00-8314-53e46ee8c282")
	)
	(pad "7" thru_hole circle
		(at 0.7 0.5)
		(size 0.4 0.4)
		(drill 0.2)
		(layers "*.Cu" "B.Mask")
		(remove_unused_layers no)
		(uuid "45dc9bc8-65c1-4c76-8a6b-fb082ecfca72")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/lib/3D/DFN2x5_6L_EP1_P.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 -0 -90)
		)
	)
)
