(footprint "NAMED_TEST_POINT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "84cdcffb-6261-470b-9564-6d528f10cd21")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "NAMED_TEST_POINT"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "2be904ff-1aeb-4896-96bc-3fa6486d8322")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c61079da-5775-46ec-82fe-c86fab3e6c05")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "98efa94d-eed0-4d73-b95b-a9f20a99dd99")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field4" "${SHORT_NET_NAME(1)}"
		(at 1 0 0)
		(layer "F.SilkS")
		(uuid "dcb66337-ddf0-4ab3-8dec-191c6c5e5462")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify left)
		)
	)
	(property "Field5" "${SHORT_NET_NAME(1)}"
		(at 1 0 0)
		(layer "B.SilkS")
		(uuid "595b6dbe-ffdc-4a36-97f7-f07b09dc03fb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify right mirror)
		)
	)
	(attr smd)
	(fp_circle
		(center 0 0)
		(end 0.8 0.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "da468c82-df61-4c22-90c6-8fed9d57d3fa")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "a9730d4f-d16e-4590-989f-4016ff05d571")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.5 1.5)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4d94f34e-83ff-4645-a457-85ccc839542b")
	)
	(embedded_fonts no)
)
