(export (version "E")
  (design
    (source "C:\\Users\\iteedi\\OneDrive - Stadlerrail AG\\Dokumente\\lasertag\\hardware\\weapon_led_board\\weapon_led_board.kicad_sch")
    (date "2026-01-05T17:05:30+0100")
    (tool "Eeschema 9.0.4")
    (sheet (number "1") (name "/") (tstamps "/")
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "weapon_led_board.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "2") (name "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/")
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "ir_led.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value "")))))
  (components
    (comp (ref "C201")
      (value "10n")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "16252c1f-69da-4f0b-ba8a-62638a07bc51"))
    (comp (ref "C202")
      (value "100n")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "d8745920-0788-4486-a16d-569d0c86ad84"))
    (comp (ref "C203")
      (value "100n")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "69371fb7-b165-47e0-b85b-8764fc73ec7b"))
    (comp (ref "C204")
      (value "10n")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "a5859203-68b2-4317-bec9-323347371559"))
    (comp (ref "C205")
      (value "1u")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "0d25d60a-7659-4564-b654-8d121dacb34f"))
    (comp (ref "C206")
      (value "10n")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "26769250-507e-4c58-95cc-2fe867bc32f9"))
    (comp (ref "D201")
      (value "LED")
      (datasheet "~")
      (description "Light emitting diode")
      (fields
        (field (name "Sim.Pins") "1=K 2=A")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Light emitting diode"))
      (libsource (lib "Device") (part "LED") (description "Light emitting diode"))
      (property (name "Sim.Pins") (value "1=K 2=A"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "LED diode"))
      (property (name "ki_fp_filters") (value "LED* LED_SMD:* LED_THT:*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "50096258-5ae9-4f1d-8b1f-cfe1238d2fb2"))
    (comp (ref "D202")
      (value "1N4148WS")
      (footprint "Diode_SMD:D_SOD-323")
      (datasheet "https://www.vishay.com/docs/85751/1n4148ws.pdf")
      (description "75V 0.15A Fast switching Diode, SOD-323")
      (fields
        (field (name "Sim.Device") "D")
        (field (name "Sim.Pins") "1=K 2=A")
        (field (name "Footprint") "Diode_SMD:D_SOD-323")
        (field (name "Datasheet") "https://www.vishay.com/docs/85751/1n4148ws.pdf")
        (field (name "Description") "75V 0.15A Fast switching Diode, SOD-323"))
      (libsource (lib "Diode") (part "1N4148WS") (description "75V 0.15A Fast switching Diode, SOD-323"))
      (property (name "Sim.Device") (value "D"))
      (property (name "Sim.Pins") (value "1=K 2=A"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "diode"))
      (property (name "ki_fp_filters") (value "D*SOD?323*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "49453426-c1a9-43fa-bb74-11faa26ad077"))
    (comp (ref "D203")
      (value "1N4148WS")
      (footprint "Diode_SMD:D_SOD-323")
      (datasheet "https://www.vishay.com/docs/85751/1n4148ws.pdf")
      (description "75V 0.15A Fast switching Diode, SOD-323")
      (fields
        (field (name "Sim.Device") "D")
        (field (name "Sim.Pins") "1=K 2=A")
        (field (name "Footprint") "Diode_SMD:D_SOD-323")
        (field (name "Datasheet") "https://www.vishay.com/docs/85751/1n4148ws.pdf")
        (field (name "Description") "75V 0.15A Fast switching Diode, SOD-323"))
      (libsource (lib "Diode") (part "1N4148WS") (description "75V 0.15A Fast switching Diode, SOD-323"))
      (property (name "Sim.Device") (value "D"))
      (property (name "Sim.Pins") (value "1=K 2=A"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "diode"))
      (property (name "ki_fp_filters") (value "D*SOD?323*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "0404c7ec-958f-4bb0-9ae3-a4f54539ca7b"))
    (comp (ref "F201")
      (value "1A")
      (datasheet "~")
      (description "Resettable fuse, polymeric positive temperature coefficient")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resettable fuse, polymeric positive temperature coefficient"))
      (libsource (lib "Device") (part "Polyfuse") (description "Resettable fuse, polymeric positive temperature coefficient"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "resettable fuse PTC PPTC polyfuse polyswitch"))
      (property (name "ki_fp_filters") (value "*polyfuse* *PTC*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "bfd1223c-b062-47ee-9538-5a6d56dc1de0"))
    (comp (ref "Q201")
      (value "AO3401A")
      (footprint "Package_TO_SOT_SMD:SOT-23")
      (datasheet "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf")
      (description "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23")
      (fields
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23")
        (field (name "Datasheet") "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf")
        (field (name "Description") "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"))
      (libsource (lib "Transistor_FET") (part "AO3401A") (description "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "P-Channel MOSFET"))
      (property (name "ki_fp_filters") (value "SOT?23*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "94dd90f5-5bb7-464a-8351-79ae0a86898d"))
    (comp (ref "Q202")
      (value "AO3400A")
      (footprint "Package_TO_SOT_SMD:SOT-23")
      (datasheet "http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf")
      (description "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23")
      (fields
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23")
        (field (name "Datasheet") "http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf")
        (field (name "Description") "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23"))
      (libsource (lib "Transistor_FET") (part "AO3400A") (description "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "N-Channel MOSFET"))
      (property (name "ki_fp_filters") (value "SOT?23*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "d8c6c0f9-47b6-49cf-b2cf-25d90865c608"))
    (comp (ref "Q203")
      (value "SS8050")
      (footprint "Package_TO_SOT_SMD:SOT-23")
      (datasheet "http://www.secosgmbh.com/datasheet/products/SSMPTransistor/SOT-23/SS8050.pdf")
      (description "General Purpose NPN Transistor, 1.5A Ic, 25V Vce, SOT-23")
      (fields
        (field (name "Sim.Device") "NPN")
        (field (name "Sim.Pins") "1=B 2=E 3=C")
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23")
        (field (name "Datasheet") "http://www.secosgmbh.com/datasheet/products/SSMPTransistor/SOT-23/SS8050.pdf")
        (field (name "Description") "General Purpose NPN Transistor, 1.5A Ic, 25V Vce, SOT-23"))
      (libsource (lib "Transistor_BJT") (part "SS8050") (description "General Purpose NPN Transistor, 1.5A Ic, 25V Vce, SOT-23"))
      (property (name "Sim.Device") (value "NPN"))
      (property (name "Sim.Pins") (value "1=B 2=E 3=C"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "SS8050 NPN Transistor"))
      (property (name "ki_fp_filters") (value "SOT?23*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "221f5692-1fac-4f23-9d17-7c82331dd911"))
    (comp (ref "Q204")
      (value "IRLR8726TRPBF")
      (footprint "Package_TO_SOT_SMD:TO-252-2")
      (fields
        (field (name "Footprint") "Package_TO_SOT_SMD:TO-252-2")
        (field (name "Datasheet"))
        (field (name "Description")))
      (libsource (lib "Transistor_FET") (part "IPD50R380CE") (description "14.1A Id, 500V Vds, CoolMOS N-Channel Power MOSFET, 380mOhm Ron, 24.8nC Qg (typ), TO-252-2"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "CoolMOS Power MOSFET N-MOS"))
      (property (name "ki_fp_filters") (value "TO?252*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "cc94161e-451b-4f43-a64d-4afe776185a5"))
    (comp (ref "Q205")
      (value "SS8050")
      (footprint "Package_TO_SOT_SMD:SOT-23")
      (datasheet "http://www.secosgmbh.com/datasheet/products/SSMPTransistor/SOT-23/SS8050.pdf")
      (description "General Purpose NPN Transistor, 1.5A Ic, 25V Vce, SOT-23")
      (fields
        (field (name "Sim.Device") "NPN")
        (field (name "Sim.Pins") "1=B 2=E 3=C")
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23")
        (field (name "Datasheet") "http://www.secosgmbh.com/datasheet/products/SSMPTransistor/SOT-23/SS8050.pdf")
        (field (name "Description") "General Purpose NPN Transistor, 1.5A Ic, 25V Vce, SOT-23"))
      (libsource (lib "Transistor_BJT") (part "SS8050") (description "General Purpose NPN Transistor, 1.5A Ic, 25V Vce, SOT-23"))
      (property (name "Sim.Device") (value "NPN"))
      (property (name "Sim.Pins") (value "1=B 2=E 3=C"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "SS8050 NPN Transistor"))
      (property (name "ki_fp_filters") (value "SOT?23*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "833deae3-478d-45ed-a718-6e9c46393391"))
    (comp (ref "Q206")
      (value "AO3400A")
      (footprint "Package_TO_SOT_SMD:SOT-23")
      (datasheet "http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf")
      (description "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23")
      (fields
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23")
        (field (name "Datasheet") "http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf")
        (field (name "Description") "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23"))
      (libsource (lib "Transistor_FET") (part "AO3400A") (description "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "N-Channel MOSFET"))
      (property (name "ki_fp_filters") (value "SOT?23*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "beccfbb2-b246-45b8-9260-3b851385a357"))
    (comp (ref "Q207")
      (value "AO3401A")
      (footprint "Package_TO_SOT_SMD:SOT-23")
      (datasheet "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf")
      (description "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23")
      (fields
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23")
        (field (name "Datasheet") "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf")
        (field (name "Description") "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"))
      (libsource (lib "Transistor_FET") (part "AO3401A") (description "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "P-Channel MOSFET"))
      (property (name "ki_fp_filters") (value "SOT?23*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "79815bda-feb1-47db-b3e7-682f83a3a87e"))
    (comp (ref "Q208")
      (value "SS8050")
      (footprint "Package_TO_SOT_SMD:SOT-23")
      (datasheet "http://www.secosgmbh.com/datasheet/products/SSMPTransistor/SOT-23/SS8050.pdf")
      (description "General Purpose NPN Transistor, 1.5A Ic, 25V Vce, SOT-23")
      (fields
        (field (name "Sim.Device") "NPN")
        (field (name "Sim.Pins") "1=B 2=E 3=C")
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23")
        (field (name "Datasheet") "http://www.secosgmbh.com/datasheet/products/SSMPTransistor/SOT-23/SS8050.pdf")
        (field (name "Description") "General Purpose NPN Transistor, 1.5A Ic, 25V Vce, SOT-23"))
      (libsource (lib "Transistor_BJT") (part "SS8050") (description "General Purpose NPN Transistor, 1.5A Ic, 25V Vce, SOT-23"))
      (property (name "Sim.Device") (value "NPN"))
      (property (name "Sim.Pins") (value "1=B 2=E 3=C"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "SS8050 NPN Transistor"))
      (property (name "ki_fp_filters") (value "SOT?23*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "770a53b1-9d30-47ca-9b27-3728d026e822"))
    (comp (ref "Q209")
      (value "SS8550")
      (footprint "Package_TO_SOT_SMD:SOT-23")
      (datasheet "http://www.secosgmbh.com/datasheet/products/SSMPTransistor/SOT-23/SS8550.pdf")
      (description "General Purpose PNP Transistor, 1.5A Ic, 25V Vce, SOT-23")
      (fields
        (field (name "Sim.Device") "PNP")
        (field (name "Sim.Pins") "1=B 2=E 3=C")
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23")
        (field (name "Datasheet") "http://www.secosgmbh.com/datasheet/products/SSMPTransistor/SOT-23/SS8550.pdf")
        (field (name "Description") "General Purpose PNP Transistor, 1.5A Ic, 25V Vce, SOT-23"))
      (libsource (lib "Transistor_BJT") (part "SS8550") (description "General Purpose PNP Transistor, 1.5A Ic, 25V Vce, SOT-23"))
      (property (name "Sim.Device") (value "PNP"))
      (property (name "Sim.Pins") (value "1=B 2=E 3=C"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "SS8550 PNP Transistor"))
      (property (name "ki_fp_filters") (value "SOT?23*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "b7d233a3-f4b9-4766-b6b6-bd3609f2c625"))
    (comp (ref "Q210")
      (value "AO3400A")
      (footprint "Package_TO_SOT_SMD:SOT-23")
      (datasheet "http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf")
      (description "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23")
      (fields
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23")
        (field (name "Datasheet") "http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf")
        (field (name "Description") "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23"))
      (libsource (lib "Transistor_FET") (part "AO3400A") (description "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "N-Channel MOSFET"))
      (property (name "ki_fp_filters") (value "SOT?23*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "f18a54ea-3763-41ae-874f-07d66f2ae977"))
    (comp (ref "R201")
      (value "10k")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "a0cad380-2cb7-4982-a015-e0807254e599"))
    (comp (ref "R202")
      (value "10k")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "9062accc-1045-4019-89e6-2dbf2e162ff1"))
    (comp (ref "R203")
      (value "10k")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "9e56d90a-da86-436d-9515-09b56f4b1d27"))
    (comp (ref "R204")
      (value "R_{SET}")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Power") "min 1W@1A!")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Power") (value "min 1W@1A!"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "d6cdf7db-3151-40a7-8313-436f58b9b71c"))
    (comp (ref "R205")
      (value "300R")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "b276ff5d-b600-47da-b49a-f5a7a5ac63f9"))
    (comp (ref "R206")
      (value "10k")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "51cfd888-ac7a-4c8b-ab3f-120717832215"))
    (comp (ref "R207")
      (value "10k")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "5b1f6f55-f8f5-4dd8-a88c-9a6a4ee33759"))
    (comp (ref "R208")
      (value "10k")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "e7be1e20-0166-4913-baf7-a10e79c70377"))
    (comp (ref "R209")
      (value "2k2")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "8956552b-a758-42a5-99fd-695ed0ee92df"))
    (comp (ref "R210")
      (value "130k")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "41627908-4d04-4b27-ac79-69293ee693ec"))
    (comp (ref "R211")
      (value "10k")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "3b2066c4-1e50-49cc-9ad1-fb718466ed69"))
    (comp (ref "R212")
      (value "1k")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "7734dc81-b8b2-44f9-ae24-3c5f760e50c8"))
    (comp (ref "R213")
      (value "10k")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "bc8d7358-831a-4c5f-8258-69031a8bcc1b"))
    (comp (ref "R214")
      (value "R_{SET OD}")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Power") "min 2W@3A!")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Power") (value "min 2W@3A!"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "f1efab9d-00e6-4c63-8894-244d4d3d8c52"))
    (comp (ref "R215")
      (value "10k")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "8772f738-086d-451f-af74-176d0c49185e"))
    (comp (ref "R216")
      (value "10k")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "db062242-54cd-4191-8a66-d3333d3b7954"))
    (comp (ref "U201")
      (value "4538")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet"))
        (field (name "Description")))
      (libsource (lib "4xxx_IEEE") (part "4538") (description ""))
      (property (name "Sheetname") (value "IR Led"))
      (property (name "Sheetfile") (value "ir_led.kicad_sch"))
      (sheetpath (names "/IR Led/") (tstamps "/cac120fb-7c47-4c6f-827d-e31e5cce535e/"))
      (tstamps "cb1a34c6-9bc4-476a-bfb6-02376189e7cf" "220824a4-2805-435e-a553-9195d3d3e61d")))
  (libparts
    (libpart (lib "4xxx_IEEE") (part "4538")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "4538")
        (field (name "Footprint"))
        (field (name "Datasheet"))
        (field (name "Description")))
      (pins
        (pin (num "1") (name "CX") (type "input"))
        (pin (num "2") (name "Rx") (type "input"))
        (pin (num "3") (name "R") (type "input"))
        (pin (num "4") (name "B") (type "input"))
        (pin (num "5") (name "A") (type "input"))
        (pin (num "6") (name "Q") (type "output"))
        (pin (num "7") (name "Q") (type "output"))
        (pin (num "8") (name "VSS") (type "power_in"))
        (pin (num "9") (name "Q") (type "output"))
        (pin (num "10") (name "Q") (type "output"))
        (pin (num "11") (name "A") (type "input"))
        (pin (num "12") (name "B") (type "input"))
        (pin (num "13") (name "R") (type "input"))
        (pin (num "14") (name "Rx") (type "input"))
        (pin (num "15") (name "CX") (type "input"))
        (pin (num "16") (name "VDD") (type "power_in"))))
    (libpart (lib "Device") (part "C")
      (description "Unpolarized capacitor")
      (docs "~")
      (footprints
        (fp "C_*"))
      (fields
        (field (name "Reference") "C")
        (field (name "Value") "C")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "Device") (part "LED")
      (description "Light emitting diode")
      (docs "~")
      (footprints
        (fp "LED*")
        (fp "LED_SMD:*")
        (fp "LED_THT:*"))
      (fields
        (field (name "Reference") "D")
        (field (name "Value") "LED")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Light emitting diode")
        (field (name "Sim.Pins") "1=K 2=A"))
      (pins
        (pin (num "1") (name "K") (type "passive"))
        (pin (num "2") (name "A") (type "passive"))))
    (libpart (lib "Device") (part "Polyfuse")
      (description "Resettable fuse, polymeric positive temperature coefficient")
      (docs "~")
      (footprints
        (fp "*polyfuse*")
        (fp "*PTC*"))
      (fields
        (field (name "Reference") "F")
        (field (name "Value") "Polyfuse")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resettable fuse, polymeric positive temperature coefficient"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "Device") (part "R")
      (description "Resistor")
      (docs "~")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "R")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "Diode") (part "1N4148WS")
      (description "75V 0.15A Fast switching Diode, SOD-323")
      (docs "https://www.vishay.com/docs/85751/1n4148ws.pdf")
      (footprints
        (fp "D*SOD?323*"))
      (fields
        (field (name "Reference") "D")
        (field (name "Value") "1N4148WS")
        (field (name "Footprint") "Diode_SMD:D_SOD-323")
        (field (name "Datasheet") "https://www.vishay.com/docs/85751/1n4148ws.pdf")
        (field (name "Description") "75V 0.15A Fast switching Diode, SOD-323")
        (field (name "Sim.Device") "D")
        (field (name "Sim.Pins") "1=K 2=A"))
      (pins
        (pin (num "1") (name "K") (type "passive"))
        (pin (num "2") (name "A") (type "passive"))))
    (libpart (lib "Transistor_BJT") (part "SS8050")
      (description "General Purpose NPN Transistor, 1.5A Ic, 25V Vce, SOT-23")
      (docs "http://www.secosgmbh.com/datasheet/products/SSMPTransistor/SOT-23/SS8050.pdf")
      (footprints
        (fp "SOT?23*"))
      (fields
        (field (name "Reference") "Q")
        (field (name "Value") "SS8050")
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23")
        (field (name "Datasheet") "http://www.secosgmbh.com/datasheet/products/SSMPTransistor/SOT-23/SS8050.pdf")
        (field (name "Description") "General Purpose NPN Transistor, 1.5A Ic, 25V Vce, SOT-23")
        (field (name "Sim.Device") "NPN")
        (field (name "Sim.Pins") "1=B 2=E 3=C"))
      (pins
        (pin (num "1") (name "B") (type "input"))
        (pin (num "2") (name "E") (type "passive"))
        (pin (num "3") (name "C") (type "passive"))))
    (libpart (lib "Transistor_BJT") (part "SS8550")
      (description "General Purpose PNP Transistor, 1.5A Ic, 25V Vce, SOT-23")
      (docs "http://www.secosgmbh.com/datasheet/products/SSMPTransistor/SOT-23/SS8550.pdf")
      (footprints
        (fp "SOT?23*"))
      (fields
        (field (name "Reference") "Q")
        (field (name "Value") "SS8550")
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23")
        (field (name "Datasheet") "http://www.secosgmbh.com/datasheet/products/SSMPTransistor/SOT-23/SS8550.pdf")
        (field (name "Description") "General Purpose PNP Transistor, 1.5A Ic, 25V Vce, SOT-23")
        (field (name "Sim.Device") "PNP")
        (field (name "Sim.Pins") "1=B 2=E 3=C"))
      (pins
        (pin (num "1") (name "B") (type "input"))
        (pin (num "2") (name "E") (type "passive"))
        (pin (num "3") (name "C") (type "passive"))))
    (libpart (lib "Transistor_FET") (part "AO3400A")
      (description "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23")
      (docs "http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf")
      (footprints
        (fp "SOT?23*"))
      (fields
        (field (name "Reference") "Q")
        (field (name "Value") "AO3400A")
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23")
        (field (name "Datasheet") "http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf")
        (field (name "Description") "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23"))
      (pins
        (pin (num "1") (name "G") (type "input"))
        (pin (num "2") (name "S") (type "passive"))
        (pin (num "3") (name "D") (type "passive"))))
    (libpart (lib "Transistor_FET") (part "AO3401A")
      (description "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23")
      (docs "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf")
      (footprints
        (fp "SOT?23*"))
      (fields
        (field (name "Reference") "Q")
        (field (name "Value") "AO3401A")
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23")
        (field (name "Datasheet") "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf")
        (field (name "Description") "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"))
      (pins
        (pin (num "1") (name "G") (type "input"))
        (pin (num "2") (name "S") (type "passive"))
        (pin (num "3") (name "D") (type "passive"))))
    (libpart (lib "Transistor_FET") (part "IPD50R380CE")
      (description "14.1A Id, 500V Vds, CoolMOS N-Channel Power MOSFET, 380mOhm Ron, 24.8nC Qg (typ), TO-252-2")
      (docs "https://www.infineon.com/dgdl/Infineon-IPD50R380CE-DS-v02_01-en.pdf?fileId=db3a30433ecb86d4013ed0a2ef580f38")
      (footprints
        (fp "TO?252*"))
      (fields
        (field (name "Reference") "Q")
        (field (name "Value") "IPD50R380CE")
        (field (name "Footprint") "Package_TO_SOT_SMD:TO-252-2")
        (field (name "Datasheet") "https://www.infineon.com/dgdl/Infineon-IPD50R380CE-DS-v02_01-en.pdf?fileId=db3a30433ecb86d4013ed0a2ef580f38")
        (field (name "Description") "14.1A Id, 500V Vds, CoolMOS N-Channel Power MOSFET, 380mOhm Ron, 24.8nC Qg (typ), TO-252-2"))
      (pins
        (pin (num "1") (name "G") (type "input"))
        (pin (num "2") (name "D") (type "passive"))
        (pin (num "3") (name "S") (type "passive")))))
  (libraries
    (library (logical "4xxx_IEEE")
      (uri "C:/Users/iteedi/OneDrive - Stadlerrail AG/Dokumente/kicad_libs/kicad-symbols/4xxx_IEEE.kicad_sym"))
    (library (logical "Device")
      (uri "C:/Users/iteedi/OneDrive - Stadlerrail AG/Dokumente/kicad_libs/kicad-symbols/Device.kicad_sym"))
    (library (logical "Diode")
      (uri "C:/Users/iteedi/OneDrive - Stadlerrail AG/Dokumente/kicad_libs/kicad-symbols/Diode.kicad_sym"))
    (library (logical "Transistor_BJT")
      (uri "C:/Users/iteedi/OneDrive - Stadlerrail AG/Dokumente/kicad_libs/kicad-symbols/Transistor_BJT.kicad_sym"))
    (library (logical "Transistor_FET")
      (uri "C:/Users/iteedi/OneDrive - Stadlerrail AG/Dokumente/kicad_libs/kicad-symbols/Transistor_FET.kicad_sym")))
  (nets
    (net (code "1") (name "GND") (class "Default")
      (node (ref "C202") (pin "2") (pintype "passive"))
      (node (ref "C203") (pin "1") (pintype "passive"))
      (node (ref "C205") (pin "2") (pintype "passive"))
      (node (ref "C206") (pin "2") (pintype "passive"))
      (node (ref "Q202") (pin "2") (pinfunction "S") (pintype "passive"))
      (node (ref "Q203") (pin "2") (pinfunction "E") (pintype "passive"))
      (node (ref "Q205") (pin "2") (pinfunction "E") (pintype "passive"))
      (node (ref "Q206") (pin "2") (pinfunction "S") (pintype "passive"))
      (node (ref "Q208") (pin "2") (pinfunction "E") (pintype "passive"))
      (node (ref "R203") (pin "2") (pintype "passive"))
      (node (ref "R204") (pin "2") (pintype "passive"))
      (node (ref "R208") (pin "1") (pintype "passive"))
      (node (ref "R213") (pin "1") (pintype "passive"))
      (node (ref "R214") (pin "2") (pintype "passive"))
      (node (ref "R215") (pin "1") (pintype "passive"))
      (node (ref "U201") (pin "8") (pinfunction "VSS") (pintype "power_in")))
    (net (code "2") (name "Net-(D201-A)") (class "Default")
      (node (ref "D201") (pin "2") (pinfunction "A") (pintype "passive"))
      (node (ref "Q201") (pin "3") (pinfunction "D") (pintype "passive")))
    (net (code "3") (name "Net-(D201-K)") (class "Default")
      (node (ref "D201") (pin "1") (pinfunction "K") (pintype "passive"))
      (node (ref "Q204") (pin "2") (pinfunction "D") (pintype "passive")))
    (net (code "4") (name "Net-(D202-A)") (class "Default")
      (node (ref "C205") (pin "1") (pintype "passive"))
      (node (ref "D202") (pin "2") (pinfunction "A") (pintype "passive"))
      (node (ref "R210") (pin "1") (pintype "passive"))
      (node (ref "U201") (pin "12") (pinfunction "B") (pintype "input")))
    (net (code "5") (name "Net-(D202-K)") (class "Default")
      (node (ref "D202") (pin "1") (pinfunction "K") (pintype "passive"))
      (node (ref "Q202") (pin "1") (pinfunction "G") (pintype "input"))
      (node (ref "R203") (pin "1") (pintype "passive"))
      (node (ref "R210") (pin "2") (pintype "passive"))
      (node (ref "U201") (pin "6") (pinfunction "Q") (pintype "output")))
    (net (code "6") (name "Net-(D203-A)") (class "Default")
      (node (ref "C203") (pin "2") (pintype "passive"))
      (node (ref "D203") (pin "2") (pinfunction "A") (pintype "passive"))
      (node (ref "R207") (pin "2") (pintype "passive"))
      (node (ref "U201") (pin "13") (pinfunction "R") (pintype "input"))
      (node (ref "U201") (pin "3") (pinfunction "R") (pintype "input")))
    (net (code "7") (name "Net-(D203-K)") (class "Default")
      (node (ref "D203") (pin "1") (pinfunction "K") (pintype "passive"))
      (node (ref "Q208") (pin "3") (pinfunction "C") (pintype "passive"))
      (node (ref "Q209") (pin "1") (pinfunction "B") (pintype "input"))
      (node (ref "R216") (pin "1") (pintype "passive")))
    (net (code "8") (name "Net-(Q201-G)") (class "Default")
      (node (ref "Q201") (pin "1") (pinfunction "G") (pintype "input"))
      (node (ref "Q202") (pin "3") (pinfunction "D") (pintype "passive"))
      (node (ref "R202") (pin "1") (pintype "passive")))
    (net (code "9") (name "Net-(Q201-S)") (class "Default")
      (node (ref "F201") (pin "2") (pintype "passive"))
      (node (ref "Q201") (pin "2") (pinfunction "S") (pintype "passive"))
      (node (ref "Q207") (pin "2") (pinfunction "S") (pintype "passive"))
      (node (ref "R202") (pin "2") (pintype "passive"))
      (node (ref "R206") (pin "2") (pintype "passive"))
      (node (ref "R209") (pin "2") (pintype "passive")))
    (net (code "10") (name "Net-(Q203-B)") (class "Default")
      (node (ref "Q203") (pin "1") (pinfunction "B") (pintype "input"))
      (node (ref "Q204") (pin "3") (pinfunction "S") (pintype "passive"))
      (node (ref "Q205") (pin "1") (pinfunction "B") (pintype "input"))
      (node (ref "Q210") (pin "3") (pinfunction "D") (pintype "passive"))
      (node (ref "R204") (pin "1") (pintype "passive")))
    (net (code "11") (name "Net-(Q203-C)") (class "Default")
      (node (ref "Q203") (pin "3") (pinfunction "C") (pintype "passive"))
      (node (ref "Q204") (pin "1") (pinfunction "G") (pintype "input"))
      (node (ref "R205") (pin "1") (pintype "passive")))
    (net (code "12") (name "Net-(Q205-C)") (class "Default")
      (node (ref "Q205") (pin "3") (pinfunction "C") (pintype "passive"))
      (node (ref "R206") (pin "1") (pintype "passive"))
      (node (ref "U201") (pin "4") (pinfunction "B") (pintype "input")))
    (net (code "13") (name "Net-(Q206-D)") (class "Default")
      (node (ref "Q206") (pin "3") (pinfunction "D") (pintype "passive"))
      (node (ref "Q207") (pin "1") (pinfunction "G") (pintype "input"))
      (node (ref "R209") (pin "1") (pintype "passive")))
    (net (code "14") (name "Net-(Q207-D)") (class "Default")
      (node (ref "Q207") (pin "3") (pinfunction "D") (pintype "passive"))
      (node (ref "R205") (pin "2") (pintype "passive")))
    (net (code "15") (name "Net-(Q208-B)") (class "Default")
      (node (ref "C206") (pin "1") (pintype "passive"))
      (node (ref "Q208") (pin "1") (pinfunction "B") (pintype "input"))
      (node (ref "Q209") (pin "3") (pinfunction "C") (pintype "passive"))
      (node (ref "R212") (pin "2") (pintype "passive"))
      (node (ref "R213") (pin "2") (pintype "passive")))
    (net (code "16") (name "Net-(Q210-S)") (class "Default")
      (node (ref "Q210") (pin "2") (pinfunction "S") (pintype "passive"))
      (node (ref "R214") (pin "1") (pintype "passive")))
    (net (code "17") (name "Net-(R212-Pad1)") (class "Default")
      (node (ref "R212") (pin "1") (pintype "passive"))
      (node (ref "U201") (pin "10") (pinfunction "Q") (pintype "output")))
    (net (code "18") (name "Net-(U201A-CX)") (class "Default")
      (node (ref "C201") (pin "2") (pintype "passive"))
      (node (ref "U201") (pin "1") (pinfunction "CX") (pintype "input")))
    (net (code "19") (name "Net-(U201A-Rx)") (class "Default")
      (node (ref "C201") (pin "1") (pintype "passive"))
      (node (ref "R201") (pin "1") (pintype "passive"))
      (node (ref "U201") (pin "2") (pinfunction "Rx") (pintype "input")))
    (net (code "20") (name "Net-(U201B-CX)") (class "Default")
      (node (ref "C204") (pin "2") (pintype "passive"))
      (node (ref "U201") (pin "15") (pinfunction "CX") (pintype "input")))
    (net (code "21") (name "Net-(U201B-Rx)") (class "Default")
      (node (ref "C204") (pin "1") (pintype "passive"))
      (node (ref "R211") (pin "1") (pintype "passive"))
      (node (ref "U201") (pin "14") (pinfunction "Rx") (pintype "input")))
    (net (code "22") (name "OUTDOOR") (class "Default")
      (node (ref "Q210") (pin "1") (pinfunction "G") (pintype "input"))
      (node (ref "R215") (pin "2") (pintype "passive")))
    (net (code "23") (name "SIGNAL") (class "Default")
      (node (ref "Q206") (pin "1") (pinfunction "G") (pintype "input"))
      (node (ref "R208") (pin "2") (pintype "passive")))
    (net (code "24") (name "VDD") (class "Default")
      (node (ref "C202") (pin "1") (pintype "passive"))
      (node (ref "F201") (pin "1") (pintype "passive"))
      (node (ref "Q209") (pin "2") (pinfunction "E") (pintype "passive"))
      (node (ref "R201") (pin "2") (pintype "passive"))
      (node (ref "R207") (pin "1") (pintype "passive"))
      (node (ref "R211") (pin "2") (pintype "passive"))
      (node (ref "R216") (pin "2") (pintype "passive"))
      (node (ref "U201") (pin "11") (pinfunction "A") (pintype "input"))
      (node (ref "U201") (pin "16") (pinfunction "VDD") (pintype "power_in"))
      (node (ref "U201") (pin "5") (pinfunction "A") (pintype "input")))
    (net (code "25") (name "unconnected-(U201A-Q-Pad7)") (class "Default")
      (node (ref "U201") (pin "7") (pinfunction "Q") (pintype "output+no_connect")))
    (net (code "26") (name "unconnected-(U201B-Q-Pad9)") (class "Default")
      (node (ref "U201") (pin "9") (pinfunction "Q") (pintype "output+no_connect")))))